Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Donning SCBA Using the Coat-Method Checklist**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Task steps** | **1 pt.** |  |
|  | **each** |  |
|  |  |  |
|  |  |  |  |

Position the SCBA with the valve end of the cylinder away from your body

Open the cylinder valve fully and acknowledge that the low-air alarm and the PASS device are activated

Check the cylinder and the remote gauge pressures and verbalize “within 100 psi” or “both gauges same pressure”

Grasp the top of the left shoulder strap on the SCBA with your left hand and raise the SCBA overhead

Guide your left elbow through the loop formed by the left shoulder strap and swing the SCBA around your left shoulder

Guide your right arm through the loop formed by the right shoulder strap allowing the SCBA to come to rest on your back

Fasten the chest strap, buckle the waist strap, and adjust the shoulder straps

Don the facepiece and check the facepiece seal

Connect the air supply to the facepiece

Activate the PASS device if it is not integrated into the system

Don the hood, helmet, and gloves

**Total points (11 possible pts.)**

Comments: